em4102-clamshell.pm3: Samy's clamshell EM4102 tag (ID: 1f00d9b3a5)
em4102-thin.pm3: Samy's thin credit-card style EM4102 tag (ID: 1a0041375d)
EM4102-1.pm3: credit card style card EM4102 tag (ID: 010872e77c)
EM4102-2.pm3: credit card style card EM4102 tag (ID: 010872beec)
EM4102-3.pm3: credit card style card EM4102 tag (ID: 010872e14f)
EM4102-Fob.pm3: (ID: 0400193cbe)
em4x05.pm3: ear tag FDX-B ISO-11784/5 (ID: 6DB0840800F80001 - Application Identifier:  8000, Country Code:  124 (Canada), National ID:  270601654)
em4x50.pm3: credit card style card EM4x50 tag (ID: DE2A3F00)
hid-proxCardII-05512-11432784-1.pm3: clamshell-style HID ProxCard II card
HID-weak-fob-11647.pm3: HID 32bit Prox Card#: 11647.  very weak tag/read but just readable.
indala-00002-12345678-1A.pm3: Indala credit-card style card
indala-504278295.pm3: PSK 26 bit indala
homeagain.pm3: HomeAgain animal (cat) tag - ID 985121004515220
homeagain1600.pm3: HomeAgain animal (cat) tag - ID 985121004515220
keri.pm3: Keri PSK-3 Key Ring tag (back of tag: 1460 3411)
lf_gprox_36_30_14489.pm3: G-Prox-II FC: 30 Card: 3949,  Format 36b  ASK/BIPHASE
lf_idteck_4944544BAC40E069.pm3:  IDTECK raw 4944544BAC40E069 , PSK,  printed  "806 082 43084"
Transit999-best.pm3: Transit 999 format (UID 99531670)
ATA5577-HIDemu-FC1-C9.pm3: ata5577 in hid prox 26 bit emulation facility code:1 card#:9
AWID-15-259.pm3: AWID FSK RF/50 FC: 15 Card: 259 
Casi-12ed825c29.pm3: casi rusco 40 bit (EM410x ID: 12ed825c29)
ioprox-XSF-01-3B-44725.pm3: IO Prox FSK RF/64 ID in name
ioprox-XSF-01-BE-03011.pm3: IO Prox FSK RF/64 ID in name
motorola_0437_00072.pm3: Motorola Grey clamshell card, old.  (RAW: A0000000E308C0C1)
nexkey_74755342.pm3:  NEXWATCH, Nexkey ID: 74755342
pac-8E4C058E.pm3: PAC/Stanley 20204/21020 PAC8 tag (ID: 8E4C058E)
quadrakey-521512301.pm3: NEXWATCH, Quadrakey ID: 521512301
securakey-64169.pm3: Securakey Tag BitLen: 26, Card ID: 64169, FC: 0x35
verichip_1022000000084146.pm3: VeriChip,  epoxy encased glasschip (ID: 1022-00000000084146) 
visa2000.pm3: VISA2000 ASK/MAN RF/64, Card: 480518
Paradox-96_40426-APJN08.pm3: PARADOX FC 96 CN 40426
TITEST.txt:  Texas Instrument - can't decode it any longer
gallagher.pm3: GALLAGHER tag.
---
sniff-ht2-BC3B8810-acg-reader.pm3:     sniffing of Hitag2 being read by an HID ACG LF Multitag reader
sniff-ht2-BC3B8810-frosch-reader.pm3:  sniffing of Hitag2 being read by a Frosch Hitag reader
sniff-ht2-BC3B8810-rfidler-reader.pm3: sniffing of Hitag2 being read by a RFIDler
---
The files 'modulation-'...
are all encoded with identical data (hex 00 01 02 03 04 05 06 07 08 09 0A 0B)
for the purpose of recognition and testing of demodulation schemes. They were created by writing Q5 tags
appropriately configured. The raw data is in 'modulation-data.dat'.
---
hf_mfu.trace:  Tracelog file for a MFU simulation
